
The HSM USB Serial Driver (Release 1.18 / Version 2.1.6.17) has been 
WHQL-certified and supports the following devices:

1. Xenon 1900 
2. Xenon 1902 
3. 3800g 
4. 4600g 
5. 4800p 
6. Honeywell Access Point
7. 4600r
8. 4800i
9. 2020 Cordless Base
10. 5180 Image Engine
11. 3800i
12. 4800dr Document Reader
13. QC890 Verifier
14. 4206
15. 5110 Image Engine
16. MS4980 Vuquest (custom f/w required to support PID 0731 - see CC#500000018288)
17. MS7580 Genesis (custom f/w required to support PID 0731 - see CC#500000018289)
18. MS7580 Genesis
19. MS9520 Voyager, MS9521 Voyager
20. MS9540 VoyagerCG, MS9541 VoyagerCG
21. MS9535 VoyagerBT
22. MS9590 VoyagerGS, MS9590i VoyagerGS, MS9591i VoyagerGS
23. MS3780 Fusion
24. MS2420 Stratos, MS2421 Stratos, MS2422 Stratos, MS2430 Stratos, MS2431 Stratos 
25. MS2320 StratosH, MS2321 StratosH, MS2322 StratosH
26. MS2122 StratosE
27. MS4980 Vuquest, MS4984 Vuquest
28. MS7820 Solaris
29. MS7600 Horizon
30. MS3580 Quantum
31. MS7120 Orbit, MS7180 OrbitCG
32. Voyager 1200g
33. Honeywell N5600 Series Area Image Engine (REM PID, PID_0974 is added)
34. Hyperion 1300
35. IS4823 Microquest Decode, IS4920 Vuquest, IS4125
37. Access Point
38. MS1690 Focus, MS1691 FocusHD, MS1633 FocusBT
39. MS5145 Eclipse
40. Voyager-1250
41. Xenon 1900P2R2
42. Xenon 1902P2R2
43. Xenon 1500
44. Vuquest 3310
45. Voyager-CCB00
46. Honeywell N8600 Series Area Image Engine
47. Voyager 1400g Series
48. 1910i Industrial Area-Imaging Scanner
49. Industrial Charge & Communication Base
50. Stratos 2700
51. Laser Engine-N4300


 *** Devices not mentioned in the list are not currently supported ***